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Product Overview
Product Introduction
	[image: D:/鑫乐视工作文档/整合/Auto Focus camera module/S5K3L8/Autofocus-S5K3L8.pngAutofocus-S5K3L8]
	XLS131796-V1.0 is a compact camera module using the S5K3L8 13MP CMOS image sensor. Featuring OmniBSI+ technology, the sensor outputs RAW images at 4208 × 3120. Image quality, data transfer and camera functions are controlled through the SCCB interface. The sensor supports up to 240 fps at full resolution.


Applications
· Barcode scanners: Used for home surveillance, video doorbells and smart locks.
· 3D scanning and QR code scanning
· Face, gesture and iris recognition
· Industrial inspection, AR/VR headsets and pattern inspection
· Pattern inspection
· High-speed image capture
Product Specifications
	Item
	Specification
	Item
	Specification

	Model
	XLS131796-V1.0
	Image Sensor
	S5K3L8

	Resolution
	4208 × 3120 (13MP)
	Optical Format
	1/3.06-inch CMOS

	Pixel Size
	1.12 μm × 1.12 μm
	Shutter Type
	Rolling shutter

	Output Format
	8-bit / 10-bit RGB RAW
	Dynamic Range
	67 dB (8× gain)

	Sensitivity
	600 mV/(lux·s)
	Maximum SNR
	34 dB

	Dark Current
	8 mV/s (50°C junction)
	Chief Ray Angle
	29.1°

	AVDD (drawing)
	2.8 V
	DOVDD (drawing)
	1.8 V

	DVDD (drawing)
	1.2 V
	Control Interface
	SCCB

	Standby Power
	35 µW
	Active Power
	198 mW

	Stable Image Junction Temp.
	0°C to 50°C
	Operating Junction Temp.
	−30°C to 70°C

	Connector
	OK-118RM024/2-35
	Input Clock
	6–27 MHz



Lens Specifications
	Item
	Specification
	Item
	Specification

	Effective Focal Length
	3.54 mm ±5%
	F-number
	2.0 ±5%

	Diagonal FOV
	78° ±3°
	Lens Construction
	5P + IR

	Distortion (drawing)
	<1%
	IR Filter
	650 nm



Maximum Sensor Frame Rates
	Mode
	Resolution
	Maximum Frame Rate

	QSXGA
	2592 × 1944
	30 fps

	1080p
	1920 × 1080
	60 fps

	960p
	960p mode
	120 fps

	720p
	1280 × 720
	120 fps

	VGA
	640 × 480
	240 fps


These are sensor-level specifications. Junction temperatures and sensor power consumption do not represent the module’s rated ambient temperature or total system power consumption. Available frame rates depend on the module configuration and host system.


Mechanical Specifications
	Item
	Specification
	Item
	Specification

	FPC Thickness
	0.15 ±0.05 mm
	Shteel Stiffener
	0.2 ±0.05 mm

	Overall Length
	17.55 ±0.2 mm
	Overall Width
	10.8 ±0.2 mm

	Overall Height
	6.2 ±0.2 mm
	Base Dimensions
	8.5 × 8.5 mm (±0.2 mm)























Product structural drawing
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Connector Pin Assignment
	Pin No.
	Signal
	I/O
	Description
	Remarks

	1
	MCLK
	input
	Clock input
	

	2
	SID(NC)
	NC
	NC
	

	3
	MDN0
	Output
	MIPI data 0 negative electrode signal
	

	4
	MDP0
	Output
	MIPI data 0 positive electrode signal
	

	5
	MDN1
	Output
	MIPI data 1 negative electrode signal
	

	6
	MDP1
	Output
	MIPI data 1 positive electrode signal
	

	7
	MCN
	Output
	MIPI clock negative electrode signal
	

	8
	MCP
	Output
	MIPI clock positive eleetrode signal
	

	9
	GND
	Ground
	Ground
	

	10
	RESET
	Input
	Reset signal input (built-up resistance, low potential)
	

	11
	SDA
	I/O
	SCCB serial interface data IO
	

	12
	SCL
	Input
	SCCB serial interface clock input
	

	13
	AVDD-2.8V
	Power
	Analog power supply 
	

	14
	AGND
	Ground
	Ground
	

	15
	VSYNC(NC)
	NC
	NC
	

	16
	AFVDD-2.8V
	Power
	AF power supply 
	

	17
	AF-GND
	Ground
	Ground
	

	18
	MDP3
	Output
	MIPI data 3 positive electrode signal
	

	19
	MDN3
	Output
	MIPI data 3 negative electrode signal
	

	20
	MDP2
	Output
	MIPI data 2 positive electrode signal
	

	21
	MDN2
	Output
	MIPI data 2 negative electrode signal
	

	22
	DGND
	Ground
	Ground
	

	23
	DOVDD-1.8V
	Power
	I/O power supply
	

	24
	DVDD-1.2V
	Power
	Digital power supply
	

	25
	
	
	
	

	26
	
	
	
	

	27
	
	
	
	

	28
	
	
	
	

	29
	
	
	
	

	30
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