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USB 720P
Camera Module

SNS-GM1084-V1.1




Supplier confirmation
	Department
	Engineer
	Quality inspector
	Approver

	Name / signature
	[LI]
	[Name / signature]
	[Name / signature]

	Date
	[26-11-05]
	[YYYY-MM-DD]
	[YYYY-MM-DD]


Customer confirmation
	Department
	Structure / appearance
	Electronics
	Approver

	Name / signature
	[Name / signature]
	[Name / signature]
	[Name / signature]

	Date
	[YYYY-MM-DD]
	[YYYY-MM-DD]
	[YYYY-MM-DD]


Contact information
SHENZHEN SINOSEEN TECHNOLOGY



[image: ]2nd Floor, Building C, Innovation Silicon Valley Industrial Park, Jingtian Road, Guanlan Guanhu Street, Longhua District, Shenzhen, China
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Revision History
	Date
	Version
	Revision Details

	2024-04-01
	V1.0
	The First Version 


	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	






Product overview
Product Introduction
	[image: 4-Lens-Sync-USB-Camera-Module-AR0144-1mp-Global-Shutter-For-Machine-Vision-2]
	SNS-GM1084-V1.1  is an 720P Ultra HD auto focus or fixed focus camera module .The maximum resolutionis 1280*800 .Support up to 720P/60 frame high-definition picture output .The
module supports USB2.0 interface,no need to install driver.The finished camera module hasthe characteristics of small size,accurate color reproduction,clear image,low power consumption andhigh reliability.



Applications
· Video conferencing
· Security and smart home
· Document cameras
· Industrial inspection
· Identity recognition
· ATMs
· Access control equipment

Product details
	Item
	Specification
	Item
	Specification

	Model
	SNS-GM1084-V1.1
	Interface
	5-pin, 1.25 mm pitch, USB 2.0

	Video output
	MJPG, YUY2
	USB signaling rate
	260 Mb/s

	Supply voltage
	5 V ±5%
	Microphone
	Dual digital noise-reduction microphone

	Operating temperature
	0°C to 50°C
	Storage temperature
	−25°C to 70°C

	Power consumption
	No LED: /
	IR LED
	/

	OS support
	Windows XP / Vista / 7 / 8 / 8.1 / 10
	Other OS support
	Mac / Android / Linux 2.6.2 (UVC) / WinCE







Chip parameters
	Item
	Specification
	Item
	Specification

	Sensor format
	1/4-inch CMOS
	Effective pixels
	1280 × 800

	Pixel size
	3.0 µm × 3.0 µm
	Sensor data output
	10-bit RAW

	Maximum SNR
	TBD
	Dynamic range
	TBD

	Minimum illumination
	TBD (no LED)
	Optical distortion
	<-1%



Lens parameters
	Item
	Specification
	Item
	Specification

	Lens mount
	/
	Construction
	4G

	F-number
	2.2 ±5%
	Effective focal length
	3.0 mm

	Field of view
	Diagonal: 68° ±3°
	Focus distance
	60 cm to infinity



Maximum frame rate
	Format
	Resolution
	Maximum frame rate

	MJPG
	1280x720  800x600  640x480  320x240
	60 fps



Product structural drawing
[image: ]

USB connector pin assignment
	Pin NO
	Pin Name
	I/O
	Description
	Remarks

	1
	VCC 5V
	P
	+5V power supply
	

	2
	D-
	A
	USB data cable-
	

	3
	D+
	A
	USB data cable+
	

	4
	GND
	G
	Ground
	

	5
	GND
	G
	Ground
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



SAMPLE APPROVAL SHEET 
SAMPLE APPROVAL SHEET 
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