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PRODUCT SPECIFICATION[image: Sinoseen company logo]

USB 16M
Camera Module

XLS-GM974-V2.0




Supplier confirmation
	Department
	Engineer
	Quality inspector
	Approver

	Name / signature
	[LI]
	[Name / signature]
	[Name / signature]

	Date
	[26-10-31]
	[YYYY-MM-DD]
	[YYYY-MM-DD]


Customer confirmation
	Department
	Structure / appearance
	Electronics
	Approver

	Name / signature
	[Name / signature]
	[Name / signature]
	[Name / signature]

	Date
	[YYYY-MM-DD]
	[YYYY-MM-DD]
	[YYYY-MM-DD]


Contact information
SHENZHEN SINOSEEN TECHNOLOGY



[image: ]2nd Floor, Building C, Innovation Silicon Valley Industrial Park, Jingtian Road, Guanlan Guanhu Street, Longhua District, Shenzhen, China



https://www.sinoseen.com/
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Revision History
	Date
	Version
	Revision Details

	2023-05-30
	V1.0
	The First Version 


	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	






Product overview
Product Introduction
	[image: D:/鑫乐视工作文档/整合/USBCamera Module/IMX298/IMX298-1.PNGIMX298-1]
	XLS-GM974-V2.0  is an 16M Ultra HD auto focus or fixed focus camera module .The maximum resolutionis 4672*3520 .Support up to 16M/30 frame high-definition picture output .The
module supports USB2.0 interface,no need to install driver.The finished camera module hasthe characteristics of small size,accurate color reproduction,clear image,low power consumption andhigh reliability.


[bookmark: _GoBack]
Applications
· Video conferencing
· Security and smart home
· Document cameras
· Industrial inspection
· Identity recognition
· ATMs
· Access control equipment

Product details
	Item
	Specification
	Item
	Specification

	Model
	XLS-GM974-V2.0
	Interface
	4-pin, 1.25 mm pitch, USB 2.0

	Video output
	MJPG, YUY2
	USB signaling rate
	260 Mb/s

	Supply voltage
	5 V ±5%
	Microphone
	Dual digital noise-reduction microphone

	Operating temperature
	0°C to 50°C
	Storage temperature
	−25°C to 70°C

	Power consumption
	No LED: /
	IR LED
	/

	OS support
	Windows XP / Vista / 7 / 8 / 8.1 / 10
	Other OS support
	Mac / Android / Linux 2.6.2 (UVC) / WinCE







Chip parameters
	Item
	Specification
	Item
	Specification

	Sensor format
	1/2.8-inch CMOS
	Effective pixels
	4672 × 3520

	Pixel size
	1.12 µm × 1.12 µm
	Sensor data output
	10-bit RAW

	Maximum SNR
	TBD
	Dynamic range
	TBD

	Minimum illumination
	TBD (no LED)
	Optical distortion
	/



Lens parameters
	Item
	Specification
	Item
	Specification

	Lens mount
	/
	Construction
	/

	F-number
	2.5 ±5%
	Effective focal length
	4.0 mm

	Field of view
	Diagonal: 76° ±3°
	Focus distance
	60 cm to infinity



Maximum frame rate
	Format
	Resolution
	Maximum frame rate

	MJPG
	2592x1944  2048x1536  1920x1200     1920x1080  1600x1200    1280x1024  1024x1024    1280x960  1280x720    1024x768  960x720    800x600  640x480    320x240  
	30 fps

	MJPG
	4656x3496  4208x3120
	5 fps



Product structural drawing
[image: ]

USB connector pin assignment
	Pin NO
	Pin Name
	I/O
	Description
	Remarks

	1
	VCC 5V
	P
	+5V power supply
	

	2
	D-
	A
	USB data cable-
	

	3
	D+
	A
	USB data cable+
	

	4
	GND
	G
	Ground
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



SAMPLE APPROVAL SHEET 
SAMPLE APPROVAL SHEET 
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