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SNS-SM1118-V1.0  /  USB 1080P CAMERA MODULE
Product overview
	
	Product description
USB 1080P camera module with a 1/3-inch progressive-scan CMOS image sensor. The source specification lists full-resolution capture at TBD fps and applications including video conferencing, surveillance, document cameras, industrial inspection, identification, ATMs and access-control equipment.


Specifications and features
USB 2.0 plug-and-play operation; still-image capture (JPG, BMP) and video capture (AVI, MP4) through the capture software. Exposure time, color difference, brightness, contrast and saturation adjustment. Progressive-scan imaging; no interpolation.
[bookmark: _GoBack]Product details
	Item
	Specification
	Item
	Specification

	Model
	SNS-SM1118-V1.0
	Interface
	5-pin, 1.25 mm USB 2.0

	Video output
	MJPG, YUY2
	USB signaling rate
	260 Mb/s

	Supply voltage
	5 V ±5%
	Microphone
	Dual digital noise-reduction microphone

	Operating temperature
	0°C to 50°C
	Storage temperature
	−25°C to 70°C

	Power consumption
	No LED: /
	IR LED
	/

	OS support
	Windows XP / Vista / 7 / 8 / 8.1 / 10
	Other OS support
	Mac / Android / Linux 2.6.2 (UVC) / WinCE


Chip parameters
	Item
	Specification
	Item
	Specification

	Sensor format
	1/3-inch CMOS
	Effective pixels
	1920× 1080

	Pixel size
	TBD
	Sensor data output
	10-bit RAW

	Maximum SNR
	TBD
	Dynamic range
	TBD

	Minimum illumination
	TBD (no LED)
	Optical distortion
	<10%


Lens parameters
	Item
	Specification
	Item
	Specification

	Lens mount
	M12 × P0.25
	Construction
	2G2P

	F-number
	2.5 ±5%
	Effective focal length
	3.0 mm

	Field of view
	Diagonal: 89° ±3°
	Focus distance
	60 cm to infinity


Maximum frame rates
	Format
	Resolution
	Maximum frame rate

	MJPG
	TBD
	TBD

	MJPG
	TBD
	TBD


TBD = to be determined. “/” indicates no value provided in the source. Frame rates above are listed for MJPG; YUY2 mode details are not supplied.


SNS-SM1118-V1.0  /  USB 1080P CAMERA MODULE
Product structural drawing
Mechanical dimensions, image orientation and connector pin assignment
[image: ]
Drawing reference
Model: SNS-SM1118-V1.0   |   Units: mm   |   Drawing date: 2026-08-27
Revision markings: V1.0 / A0   |   Unspecified dimensional tolerance: ±0.1 mm
USB connector pin assignment
	Pin
	1
	2
	3
	4
	5

	Signal
	USB+5V
	DM/D−
	DP/D+
	GND
	GND


The structural drawing is retained from the source specification. Refer to the dimensioned drawing for assembly and inspection.
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Product appearance specifications
Appearance inspection
	#
	Item
	Requirements
	Test method
	Class

	1
	Module appearance
	No surface dirt, no scratches visible to the naked eye, and no impurities in the plastic.
	8× magnifier
	A

	2
	Lens
	No visible scratches or dirt under 800 ±100 lux illumination, viewed head-on and with 45° reflected light.
	8× magnifier
	A

	3
	Thread adhesive
	Adhesive length: 1/3 to 1/2 of the circumference. Adhesive must not overflow onto the lens end face or lens base.
	8× magnifier
	A

	4
	Sealant
	Apply evenly between the base and PCB, without gaps or uneven thickness. No overflow beyond the FPC edge that causes the assembly dimensions to exceed the specified limits.
	8× magnifier
	A

	5
	PCB
	Surface clean; printed characters legible. Edge burr: length <1 mm, width <0.3 mm. Edge notch: length <1 mm, width <0.1 mm; no more than 2 notches per edge.
	45× microscope
(continuous zoom)
	A


Dimensional inspection
	#
	Item
	Requirements
	Test method
	Class

	1
	Height
	Conform to the product drawing.
	Digital caliper
	A

	2
	Length
	Conform to the product drawing.
	Digital caliper
	A

	3
	Width
	Conform to the product drawing.
	Digital caliper
	A


Defect classes A and B are defined on the following page.
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Product image specifications
Optical performance inspection requirements
	#
	Test item
	Requirements
	Test method
	Class

	1
	Dust
	No visible foreign objects anywhere in the captured white-field image.
	Test fixture; small light box; 6500 K white backlight
	A

	2
	Image orientation
	Conform to the product drawing.
	Test fixture
	A

	3
	Bright and dark pixels
	Dark field: <400 bright pixels; <20 two-adjacent-pixel bright clusters; no bright clusters of more than 3 pixels. White field: <400 dark pixels; <20 two-adjacent-pixel dark clusters; no dark clusters of more than 3 pixels.
	Test software; small light box; 6500 K white backlight
	A

	4
	Resolution
	1080P: center resolution ≥500 LW/PH.
	MTF test procedure
	A

	5
	FOV
	Diagonal: 89° ±3°.
	Test fixture; FOV reference board
	A

	6
	Shading
	At the four corner positions described as “90% away from the center”: mean corner brightness ≥45% of center brightness; each corner >35% of center. Sampling window: 40 × 40 pixels; sensor vignetting compensation disabled.
	Test software; small light box; 3400 lux, 6500 K white backlight
	A

	7
	Color
	Color reproduction error ≤20%.
	Test software; color checker
	A

	8
	TV distortion
	Pincushion (+) or barrel (−) distortion: no more than 1%.
	Test software; ISO 12233 chart
	A

	9
	Grayscale
	Brightness difference between adjacent gray levels <8.
	Test software; grayscale chart
	A

	10
	CA
	<0.5.
	Test software; ISO 12233 chart
	A

	11
	Torque
	≥0.5 kgf·cm.
	Torque wrench
	A

	12
	Thrust
	≥2 N.
	Thrust gauge
	A


Defect classification
A — Major nonconformity: affects image quality, principal functions or performance specifications, or results in rejection of the inspected batch.
B — General nonconformity: does not affect final product appearance, technical performance, or subsequent processing and assembly.
Source criteria retained. CA units, grayscale calculation, color-error method and the exact shading measurement positions require engineering confirmation before customer approval.
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Product sampling plan
Imaging and reliability
	#
	Test item
	Sampling plan
	Test method / remarks

	1
	Dust
	Each batch: N=5, C=0
	Same as production; production inspection

	2
	Image orientation
	Each batch: N=5, C=0
	Test fixture; production inspection

	3
	Bright and dark pixels
	Each batch: N=5, C=0
	Same as production; production inspection

	4
	Resolution
	Each batch: N=5, C=0
	MTF test procedure; production inspection

	5
	FOV
	Each batch: N=5, C=0
	Test fixture / FOV board; QA sampling and full evaluation at sample stage

	6
	Image uniformity
	Each batch: N=5, C=0
	Test software; 3400 lux, 6500 K light box; production inspection

	7
	Dispersion
	Each batch: N=5, C=0
	Test software / color checker; QA sampling and full evaluation at sample stage

	8
	TV distortion
	Each batch: N=5, C=0
	Test software / ISO 12233 chart; QA sampling and full evaluation at sample stage

	9
	Grayscale
	Each batch: N=5, C=0
	Test software / grayscale chart; QA sampling and full evaluation at sample stage

	10
	Reliability
	Trial production: 2 pcs / production batch. Stable production: 5 pcs / test item / month.
	Acceptance level: 0/1, as stated in the source.


Appearance
	#
	Test item
	Sampling plan
	Test method / remarks

	1
	Module appearance
	AQL=1.0
	Visual; production inspection

	2
	Lens
	AQL=1.0
	8× magnifier; production inspection

	3
	Thread adhesive
	AQL=1.0
	8× magnifier; production inspection

	4
	Sealant
	AQL=1.0
	8× magnifier; production inspection

	5
	FPC
	AQL=1.0
	Visual; production inspection

	6
	Gold fingers
	AQL=1.0
	Visual; production inspection

	7
	Steel stiffener
	AQL=1.0
	Visual; production inspection

	8
	Double-sided tape
	AQL=1.0
	Visual; production inspection


Dimensions and mechanical checks
	#
	Test item
	Sampling plan
	Test method / remarks

	1
	Height
	AQL=1.0
	Same as production; production inspection

	2
	Length
	AQL=1.0
	Same as production; production inspection

	3
	Width
	AQL=1.0
	Same as production; production inspection

	4
	Thread torque
	Each batch: N=5, C=0
	Torque wrench; QA sampling

	5
	Base thrust
	Each batch: N=5, C=0
	Thrust gauge; QA sampling


N = sample size; C = acceptance number. AQL values are reproduced from the source; the governing sampling standard and inspection level are not specified.
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Product reliability specifications
	#
	Test item
	Conditions and requirements
	Test equipment

	1
	Low-temperature storage
	−30°C for 48 h. Return to room temperature for 2 h before testing.
	Low-temperature chamber + computer

	2
	Low-temperature operation
	−20°C; operate the product and inspect the image for 48 h.
	Low-temperature chamber + computer

	3
	High-temperature storage
	80°C for 48 h. Return to room temperature for 2 h before testing.
	High-temperature chamber + computer

	4
	High-temperature operation
	70°C; operate the product and inspect the image for 48 h.
	High-temperature chamber + computer

	5
	Aging
	Operate at room temperature for 36 h and check for image abnormalities.
	Computer

	6
	Connector mating
	Connector plugging / unplugging. Cycle count and detailed conditions are not specified in the source.
	Workbench + computer

	7
	Electrostatic discharge
	Apply ±6 kV contact discharge and ±8 kV air discharge at the exposed copper grounding location. Apply 10 discharges per polarity at each point, with a 1 s interval.
	ESD equipment + computer

	8
	Free drop after packaging
	Drop the packaged product freely from 150 cm, then check the image.
	Oak floor + computer

	9
	Vibration after packaging
	Fix the packaged product to the test bench. Sweep 10–100–10 Hz; amplitude 2 mm; X, Y and Z directions; test duration 2 h as stated in the source. Check the image after testing.
	Vibration test bench + computer


Acceptance requirements
After the reliability tests, dimensions, appearance, torque and optical performance must conform to the product requirements.
Post-test inspection conditions
	Item
	Condition

	Small light box
	1500 lux ±10%

	Large light box
	6000 lux ±10%

	Color temperature
	4400 K ±150 K

	Inspection system
	PC test software / module test platform


Reliability test conditions are reproduced from the source and do not extend the rated operating or storage ranges on page 2. This page defines test requirements, not a completed test report.
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