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1  Controller Overview
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Smart Controller key layout
	Key
	Main functions

	Left key
	Select the previous menu item. During heating, increase the level or target temperature. During setup, adjust the flashing value as indicated on screen.

	Right key
	Select the next menu item. During heating, decrease the level or target temperature. During ventilation time setup, increase the running time; use the on-screen value to confirm direction in other setup menus.

	Return key
	Return to the previous menu. Press and hold for 3 seconds during operation to switch between manual output mode and thermostat mode.

	Power/OK key
	Confirm a selection, enter a menu and start a function. Press and hold for approximately 3 seconds to stop heating or ventilation.



2  First Power-Up and Main Interface
	1
	Connect power to the heater and controller.



	2
	The screen opens at the time-setting interface. Press Power/OK to confirm or enter the week setting.



	3
	Press Power/OK again to open the main interface.



	4
	Use the Left and Right keys to move between Heating, Ventilation, Timer and Settings.



	5
	When the required icon flashes, press Power/OK to enter that function.



	Standby shortcut: From the main interface in standby, short-press Power/OK to enter the heating run-time setting. Press Power/OK again to start heating.



3  Heating Operation
3.1 Start heating
	1
	Select the heating icon and press Power/OK.



	2
	Set the operating time with the Left/Right keys. The selectable range is 10-120 minutes. After 120 minutes, the next setting is continuous operation (∞).



	3
	Press Power/OK to start heating.



	4
	Use the Left key to increase and the Right key to decrease the manual output level or thermostat temperature.



3.2 Stop heating
	1
	Press and hold Power/OK for approximately 3 seconds.



	2
	The display shows OFF and the heater begins its automatic shutdown and cool-down cycle.



	3
	Wait until the heater has completely stopped before disconnecting the power supply.



	After-run protection: Do not use a battery isolator or disconnect the supply during normal shutdown. Interrupting the after-run cycle can damage the heater.



4  Ventilation Mode
	1
	On the main interface, select the FAN icon and press Power/OK.



	2
	Set the running time. In the current controller instructions, the Left key reduces the time and the Right key increases it.



	3
	Press Power/OK to begin ventilation.



	4
	Adjust fan speed from L1 to L10 with the Left and Right keys.



	5
	To stop ventilation, press and hold Power/OK for approximately 3 seconds. The controller returns to the main interface.



5  Manual/Thermostat Mode
	Operating state
	Action
	Display result

	Heater running
	Press and hold Return for 3 seconds.
	Thermostat mode is active when a target temperature such as 30 °C appears in the upper-right corner.

	Thermostat mode active
	Press and hold Return for 3 seconds again.
	Manual mode is active when a level such as L4 is displayed. Manual mode is the default.

	Using remote control
	Press and hold the remote-control power key for 3 seconds.
	The controller cycles between manual and thermostat mode. Wait more than 3 seconds before switching again.



6  Remote Control Pairing
	1
	Place the heater in standby.



	2
	Press and hold the Left key and Return key together for 3 seconds to open the remote-pairing interface.



	3
	Press and hold the power key on the remote control.



	4
	After successful pairing, the controller exits the pairing interface automatically.



	5
	To cancel, short-press Power/OK. The controller also exits automatically after approximately 20 seconds without input.



One Smart Controller can be paired with up to two remote controls.
7  Fuel Priming
	Use only when required: Priming is intended for the initial fuel-line fill after the power supply is connected. Excessive priming can introduce too much fuel into the heater.



	1
	With the heater in standby, press and hold the Right key for 3 seconds.



	2
	When the display shows Priming, press Power/OK to start.



	3
	After successful ignition, the heater enters normal operation.



	4
	Priming can be used only once after the first power connection. To use it again, disconnect and reconnect the power supply.



8  Time and Date
	1
	In standby, select the Settings icon with the Left/Right keys and press Power/OK.



	2
	Select the flashing clock icon and press Power/OK.



	3
	Set the hour in 24-hour format with the Left/Right keys, then press Power/OK.



	4
	Set the minutes and press Power/OK.



	5
	Select the day of the week: MON, TUE, WED, THU, FRI, SAT or SUN.



	6
	Press Return to go back, or Power/OK to return to the main interface.



9  Timer Programs P1-P3
The controller provides three programmable start times. P1, P2 and P3 may be set for the same day or for different days.
	1
	On the main interface, select the P timer icon and press Power/OK.



	2
	Select P1, P2 or P3, then press Power/OK.



	3
	Select the day of the week and press Power/OK.



	4
	Set the start hour and minute, confirming each field with Power/OK.



	5
	Set the running time from 10-120 minutes or continuous operation (∞).



	6
	Select ON or OFF with the Left/Right keys and confirm.



	7
	Press Return to return to the main interface.



	Timer status: When a timer is enabled, the timer icon appears and the active program is marked. After a programmed operation finishes, the check mark for that program is cleared.



10  Status Display
	1
	While the heater is running, press and hold the Left and Right keys together.



	2
	The status interface displays power-supply voltage, motor speed (RPM), fuel-pump frequency and Alpine elevation data.



	3
	Use the Left or Right key to change pages.



11  Screen-Off State
The screen turns off after approximately 3 minutes without key operation, both in standby and during operation. If an indicator is blinking while the screen is off, press any key to wake the controller.


12  Safe Operation Notes
After a long period of non-use, check that the heater and accessories are securely mounted.
Inspect the fuel system visually for leaks and use fresh fuel where possible.
Pro Max 2 kW Alpine heaters adjust automatically from sea level to 3,000 m (9,842 ft).
Pro Max 5 kW Alpine heaters adjust automatically from sea level to 5,500 m (18,044 ft).
No owner altitude adjustment is required on Alpine versions.
When a fault code appears, correct the fault before clearing the display. Refer to the separate Error Codes List.
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